**Assignment-4**

|  |  |
| --- | --- |
| Assignment Date | 22October 2022 |
| Student Name | Mr KISHORE A B |
| Student Roll Number | 732919ECR074 |
| Maximum Marks | 2 Marks |

**Question 1**:

Write a code and connections in wokwi for the ultrasonic sensor. Whenever the distance is less than 100cms send an “Alert” to IBM cloud and display in the device recent events.

**Solution:**

# Coding:

#include<WiFi.h>

#include<PubSubClient.h>

WiFiClientwifiClient;

String data3;

#define ORG "w63fd1"

#define DEVICE\_TYPE "JehoNi"

#define DEVICE\_ID "123"

#define TOKEN "12345678"

#define speed 0.034#define led 14char server[] = ORG "[.messaging.internetofthings.ibmcloud.com"](http://messaging.internetofthings.ibmcloud.com/); charpublishTopic[] = "iot-2/evt/Data/fmt/json"; char topic[] = "iot-2/cmd/command/fmt/String"; charauthMethod[] = "use-token-auth"; char token[] = TOKEN; charclientId[] = "d:" ORG ":"DEVICE\_TYPE ":" DEVICE\_ID; PubSubClient client(server, 1883, wifiClient); voidpublishData();

constinttrigpin=5; constintechopin=18; String command;

String data="";

long duration; floatdist;

voidsetup()

{

**Serial**.begin(115200); pinMode(led, OUTPUT); pinMode(trigpin, OUTPUT); pinMode(echopin, INPUT); wifiConnect(); mqttConnect();

}

voidloop() { boolisNearby = dist<100; digitalWrite(led, isNearby);

publishData(); delay(500);

if(!client.loop()) { mqttConnect();

}

}

voidwifiConnect() {

**Serial**.print("Connecting to "); **Serial**.print("Wifi"); WiFi.begin("Wokwi-GUEST", "", 6); while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.print("WiFi connected, IP address: ");

**Serial**.println(WiFi.localIP());

}

voidmqttConnect() { if (!client.connected()) {

**Serial**.print("Reconnecting MQTT client to "); **Serial**.println(server); while (!client.connect(clientId, authMethod, token)) { **Serial**.print("."); delay(500);

} initManagedDevice();

**Serial**.println();

}

}

voidinitManagedDevice() { if (client.subscribe(topic)) {

// Serial.println(client.subscribe(topic));

**Serial**.println("IBM subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

} }voidpublishData()

{ digitalWrite(trigpin,LOW); digitalWrite(trigpin,HIGH); delayMicroseconds(10); digitalWrite(trigpin,LOW); duration=pulseIn(echopin,HIGH); dist=duration\*speed/2; if(dist<100){

String payload = "{\"Normal Distance\":";

payload += dist; payload += "}";

**Serial**.print("\n");

**Serial**.print("Sending payload: "); **Serial**.println(payload); if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish OK");

}

} if(dist>101&&dist<111){

String payload = "{\"Alert distance\":"; payload += dist;

payload += "}";

**Serial**.print("\n");

**Serial**.print("Sending payload: "); **Serial**.println(payload); if(client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Warning crosses 110cm -- it automaticaly of the loop"); digitalWrite(led,HIGH);

}else {

**Serial**.println("Publish FAILED");

}

}

}

voidcallback(char\* subscribeTopic, byte\* payload, unsignedintpayloadLength){

**Serial**.print("callback invoked for topic:");

**Serial**.println(subscribeTopic);

for(inti=0; i<payloadLength; i++){ dist += (char)payload[i];


}


**Serial**.println("data:"+ data3); if(data3=="lighton"){ **Serial**.println(data3); digitalWrite(led,HIGH);

} data3="";

}

## OUTPUT-Wokwi





**OUTPUT-cloud**

